Stoddard Mississippi USGS Corrections

UTM 15

-In the original delivery 18 .las files were delivered for the 16 delivery tiles.



We are redelivering the 16 .las files intended for the Stoddard Mississippi UTM 15 delivery.

UTM 16

-Several Linear anomalies were measured less than 10 cm and in some cases less than 5 cm. These anomalies are considered to be within flightline to flighline tolerance.

-There is an edit call for a median to be removed from the ground class.

This median is low to the ground, almost like a curb, and has remained in the ground class.




-Edit call Hydorflattening\_2

The hydro was processed separately because the LiDAR was acquired on different dates where the water level was different.


-There is an edit call referring to steep banks on a pond.

The banks for the pond actually steep.

Hydro flattened DEM:



Unprocessed Bare Earth DEM:



-Classified .las files for tiles 299\_4089 and 299\_4093 have been recreated.