From: DAS

To: USGS (QC Team)

Date: 10/20/2016

Subject: Replacement DEM: FY16\_NRCS Arkansas-QL2 LiDAR-Delivery One

The dataset located on drive: [IN0030:\FY16\_NRCS\_Arkansas\_QL2\_LiDAR\First\_Deliverable\_Update](file:///H%3A%5CFY16_NRCS_Arkansas_QL2_LiDAR%5CFirst_Deliverable_Update) are replacement BareEarth-DEM for four tiles affected by erroneous Breakline (pond) elevation in the first delivery dataset. This error has been fixed, hence the need to replace the four affected DEM & Breakline (Ponds\_Lakes).

Image 01: DEM Artifact due to Erroneous Pond Elevation



Image02: DEM Error Fixed

