{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["FlightLog"],"not_rendered":{"charts":0,"images":7,"macros":1,"external_links":0,"defined_names":3,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"FlightLog","index":0,"n_rows":38,"n_cols":31,"rows_kept":38,"cut":false,"hidden":false,"merged":[[3,15,3,16],[15,3,15,4],[0,14,0,18],[2,15,2,16],[3,17,3,18],[2,17,2,18],[7,0,7,1],[8,2,8,3],[8,0,8,1],[7,2,7,3],[0,3,0,6],[2,9,2,10],[3,9,3,10],[0,7,0,8],[5,0,5,1],[6,12,6,13],[6,10,6,11],[6,2,6,7],[5,16,5,17],[5,8,5,9],[6,8,6,9],[5,12,5,13],[5,10,5,11],[6,16,6,17],[31,15,31,24],[28,15,28,24],[29,15,29,24],[32,15,32,24],[35,15,35,24],[19,15,19,24],[22,15,22,24],[23,15,23,24],[20,15,20,24],[21,15,21,24],[34,15,34,24],[24,15,24,24],[25,15,25,24],[27,15,27,24],[26,15,26,24],[33,15,33,24],[37,15,37,24],[23,11,23,12],[28,8,28,9],[28,11,28,12],[24,11,24,12],[25,11,25,12],[23,8,23,9],[7,5,7,6],[8,5,8,6],[12,3,12,6],[10,0,10,4],[25,8,25,9],[24,8,24,9],[12,0,12,2],[21,11,21,12],[22,8,22,9],[20,8,20,9],[21,8,21,9],[15,5,15,6],[14,1,14,4],[13,5,13,6],[15,1,15,2],[17,11,17,12],[30,15,30,24],[9,5,9,6],[10,5,10,6],[14,5,14,6],[7,12,7,14],[7,15,7,17],[9,11,9,12],[8,12,8,14],[8,10,8,11],[13,14,13,17],[12,7,12,10],[14,14,14,17],[11,3,11,6],[13,1,13,4],[14,8,14,9],[10,11,10,12],[9,15,9,17],[9,0,9,4],[8,7,8,9],[7,7,7,9],[11,15,11,26],[12,15,12,26],[14,25,14,26],[7,23,7,26],[7,18,7,19],[15,27,16,27],[13,18,13,21],[14,18,14,21],[8,27,8,29],[9,20,9,21],[10,23,10,26],[8,18,8,19],[8,23,8,26],[9,23,9,26],[13,25,13,26],[14,22,14,24],[15,15,16,24],[13,22,13,24],[8,15,8,17],[16,11,16,12],[10,15,10,17],[19,11,19,12],[3,11,3,12],[4,17,4,18],[36,8,36,9],[36,11,36,12],[37,8,37,9],[37,11,37,12],[15,7,15,9],[19,8,19,9],[10,8,10,9],[9,8,9,9],[13,8,13,9],[35,8,35,9],[35,11,35,12],[34,8,34,9],[34,11,34,12],[30,8,30,9],[30,11,30,12],[33,8,33,9],[33,11,33,12],[31,8,31,9],[36,15,36,24],[4,9,4,10],[1,9,1,10],[5,20,5,21],[26,8,26,9],[26,11,26,12],[17,8,17,9],[32,8,32,9],[32,11,32,12],[27,11,27,12],[11,7,11,10],[11,11,11,14],[18,11,18,12],[31,11,31,12],[27,8,27,9],[29,8,29,9],[29,11,29,12],[12,11,12,14],[15,11,15,12],[18,8,18,9],[16,8,16,9],[17,15,17,24],[18,15,18,24],[22,11,22,12],[20,11,20,12],[0,22,0,23],[1,22,1,23],[2,22,2,23],[3,22,3,23],[1,17,1,18],[14,10,14,13],[13,10,13,13],[6,0,6,1],[7,20,7,21],[11,0,11,2],[6,23,6,26],[5,2,5,7],[7,10,7,11],[0,24,1,26],[2,24,3,26],[4,24,4,26],[1,11,1,12],[4,22,4,23],[5,23,5,26],[2,11,2,12],[4,11,4,12],[4,15,4,16],[1,15,1,16],[0,9,0,13]]}
["ALS",{"$f":"AC1","v":19.023},"FHI","Fugro Geospatial",null,null,null,{"$f":"B1","v":19.023},null,"Lift Begin",null,null,null,null,"Lift End",null,null,null,null,"Flt","Flt ","Hobbs",null,null," ALS",null,null,"AO80-44-00-02",19.023,"2019-01-23","Jerry"]
[null,null,null,null,null,null,null,null,null,"Airport",null,"Chocks",null,"Hobbs","Airport","Chocks",null,"Hobbs",null,"Duration","Hrs","Hrs","   Actvity",null,null,null,null,"ISO #","Ver","Date","By"]
[null,null,null,null,null,null,null,null,1,"KLMU",null,"18:39:23",null,3129.7,"KLMU","22:47:29",null,3133.4,null,{"$f":"IF(P3=\"\",\"\",IF(P3<L3,P3+1,P3)-L3)","v":"04:08:06"},{"$f":"IF(T3=\"\",\"\",(INT(((INT(T3*1440+1/60))+7)/15)*15)/60)","v":4.25},{"$f":"IF(R3=\"\",\"\",R3-N3)","v":3.7000000000002728},"0900-Production",null,"Flight Log"]
[null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(P4=\"\",\"\",IF(P4<L4,P4+1,P4)-L4)","v":""},{"$f":"IF(T4=\"\",\"\",(INT(((INT(T4*1440+1/60))+7)/15)*15)/60)","v":""},{"$f":"IF(R4=\"\",\"\",R4-N4)","v":""}]
[null,null,null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(P5=\"\",\"\",IF(P5<L5,P5+1,P5)-L5)","v":""},{"$f":"IF(T5=\"\",\"\",(INT(((INT(T5*1440+1/60))+7)/15)*15)/60)","v":""},{"$f":"IF(R5=\"\",\"\",R5-N5)","v":""},null,null,"AO80-44-00-02"]
["FGI Job #",null,"Project Name",null,null,null,null,null,"System",null,"Unit",null,"IMU",null,"PiA","SW1","SW2-Gain",null,"Aper","AutoScan","Ground Temp°C",null,"Min Range Gate","Data Logger Drive"]
["04.33780163",null,"CPRA LADOTD",null,null,null,null,null,"ALS80",null,118,null,"uIRS",null,6,"","",null,60,"Yes",24,26,"2657m","MM70-01"]
["Flight Date",null,"GPS Day",null,"Lift",null,null,null,null,null,"Sun°",null,"Solar Times (UTC)",null,null,"Laser Power",null,null,"Pattern",null,"Flying Temp °C",null,"Max Range Gate","Download Drive"]
["2019-04-26",null,{"$f":"IF(ISBLANK(A9),\" \",CONCATENATE(TEXT(MOD(YEAR(A9),100),\"00\"),\"-\",TEXT(INT(A9)+1-DATEVALUE(CONCATENATE(\"1-Jan-\",YEAR(A9))),\"000\")))","v":"19-116"},null,15,null,null,null,null,null,"NA",null,"NA",null,null,1,null,null,"Triangle",null,8,9,"2931m","NS1TB-96"]
["Mission ID    (yymmdd_Sen_Job_Lift)",null,null,null,null,"Aircraft",null,"Airport ID","FMS",null,"UTC","AMT (ft)",null,"Speed","Scan Hz","Pulse Rate",null,null,"FOV","km/WPT","Altm Setting",null,null,"Shipping Track"]
["190426_118_33780163_15",null,null,null,null,"N8131",null,"KLMU","CCNS 4",null,"",9101,null,150,53,610000,null,null,"",1.6679999999999999,30.11,30.06,null,"7750 7712 6012"]
["Pilot #1",null,null,"Pilot #2",null,null,null,"Operator #1",null,null,null,"Operator #2"]
["Wayne Manning",null,null,"",null,null,null,"Dave Verhey",null,null,null,""]
["Base 1 ID","Location",null,null,null,"Rec ID",null,"Ant ID","ARP (m)",null,"Start Time (UTC)",null,null,null,"Stop Time (UTC)",null,null,null,"GPS Filename",null,null,null,"Operator",null,null,"Data"]
["FUG-KLMU","KLMU",null,null,null,"GR3U7",null,"U7",1.8,null,"2019-04-26T18:13:00",null,null,null,"2019-04-26T22:59:00",null,null,null,"unit70426s",null,null,null,"CORS",null,null,"FTP"]
["   ","Flight #",null,"Wpt",null,"Distance",null,"UTC",null,null,"Flt","Altitude",null,"Speed","Scan","Comments and Conditions",null,null,null,null,null,null,null,null,null,"   ",null,"OnLine Time"]
["Area","FGI","Client's","From","To","Begin","End","Start","End",null,"Dir","(GPS)",null,"(knots)","Rate",null,null,null,null,null,null,null,null,null,null,"SVs","PDOP"]
[null,null,null,null,null,null,null,"18:41:36","18:46:36",null,null,null,null,null,null,"Ground Static at KLMU",null,null,null,null,null,null,null,null,null,20,1.3,{"$f":"IF(H18=\"\",0,IF(I18=\"\",0,I18-H18))","v":"00:05:00"}]
[null,null,null,null,null,null,null,"19:17:57","19:20:13",null,null,null,null,null,null,"S-Turn",null,null,null,null,null,null,null,null,null,19,1.2,{"$f":"IF(H19=\"\",0,IF(I19=\"\",0,I19-H19))","v":"00:02:16"}]
["LA_1X",10,null,26,37,42,60,"19:23:52","19:28:08",null,"90.1",9160,null,130,null,"Tie line.",null,null,null,null,null,null,null,null,null,17,1.3,"00:04:16"]
["LA_1C",79,null,31,1,50,0,"19:32:59","19:44:47",null,"180.1",9051,null,146,null,"Excess roll at 15 km. Water 15.5-5.5 km",null,null,null,null,null,null,null,null,null,17,1.3,"00:11:48"]
[null,78,null,1,31,0,50,"19:49:31","20:01:21",null,"0.1",9138,null,135,null,"Water 11-16 km.",null,null,null,null,null,null,null,null,null,19,1.3,"00:11:50"]
[null,78,null,31,22,50,35,"20:05:18","20:08:59",null,"180.1",9015,null,147,null,"Calibration line.",null,null,null,null,null,null,null,null,null,19,1.1000000000000001,"00:03:41"]
[null,null,null,null,null,null,null,"20:19:49","20:21:25",null,null,null,null,null,null,"S-Turn",null,null,null,null,null,null,null,null,null,20,1.1000000000000001,"00:01:36"]
[null,77,null,31,1,50,0,"20:23:17","20:34:47",null,"180.1",9091,null,147,null,"Water 15-9, 7, 2.5-0.5 km.",null,null,null,null,null,null,null,null,null,20,1.1000000000000001,"00:11:30"]
[null,76,null,1,31,0,50,"20:39:33","20:51:20",null,"0.1",9101,null,142,null,"Water 1-2.5, 12.5-15 km.",null,null,null,null,null,null,null,null,null,20,1.2,"00:11:47"]
[null,75,null,31,1,50,0,"20:55:14","21:07:20",null,"180.1",9061,null,140,null,"Water 15.5-13 km; excess roll 11 km; Water 1.5-0.5 km",null,null,null,null,null,null,null,null,null,20,1.1000000000000001,"00:12:06"]
[null,74,null,1,31,0,50,"21:11:20","21:22:46",null,"0.1",9098,null,143,null,"Water 1, 9.5, 13.5-16.5 km",null,null,null,null,null,null,null,null,null,20,1.1000000000000001,"00:11:26"]
[null,73,null,31,1,50,0,"21:26:08","21:37:48",null,"180.1",9092,null,140,null,"Water 16-13 km; course correction at 9.5; severe course correction 6 km; water 1 km",null,null,null,null,null,null,null,null,null,20,1.1000000000000001,"00:11:40"]
[null,72,null,1,31,0,50,"21:43:56","21:55:36",null,"0.1",9139,null,141,null,"Water 1, 15-17 km; sudden roll 32 km.",null,null,null,null,null,null,null,null,null,18,1,"00:11:40"]
[null,71,null,31,1,50,0,"21:59:47","22:11:07",null,"180.1",9116,null,147,null,"Water 16.5-15, 1.5-0 km",null,null,null,null,null,null,null,null,null,18,1.1000000000000001,"00:11:20"]
[null,70,null,1,31,0,50,"22:15:23","22:15:35",null,"0.1",null,null,null,null,"Line aborted for traffic.",null,null,null,null,null,null,null,null,null,16,1.4,"00:00:12"]
[null,null,null,null,null,null,null,"22:21:17","22:23:12",null,null,null,null,null,null,"S-Turn",null,null,null,null,null,null,null,null,null,16,1.3,"00:01:55"]
[null,null,null,null,null,null,null,"22:39:17","22:44:17",null,null,null,null,null,null,"Ground Static at KLMU",null,null,null,null,null,null,null,null,null,17,1.3,"00:05:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"00:00:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H37=\"\",0,IF(I37=\"\",0,I37-H37))","v":"00:00:00"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H38=\"\",0,IF(I38=\"\",0,I38-H38))","v":"00:00:00"}]