{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["FlightLog"],"not_rendered":{"charts":0,"images":7,"macros":1,"external_links":0,"defined_names":3,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"FlightLog","index":0,"n_rows":38,"n_cols":31,"rows_kept":38,"cut":false,"hidden":false,"merged":[[0,14,0,18],[2,15,2,16],[3,17,3,18],[2,17,2,18],[7,0,7,1],[8,2,8,3],[8,0,8,1],[7,2,7,3],[0,3,0,6],[2,9,2,10],[3,9,3,10],[0,7,0,8],[5,0,5,1],[5,2,5,7],[1,11,1,12],[2,11,2,12],[4,15,4,16],[1,15,1,16],[0,9,0,13],[3,11,3,12],[4,17,4,18],[4,9,4,10],[1,9,1,10],[7,5,7,6],[34,15,34,24],[21,15,21,24],[24,15,24,24],[25,15,25,24],[22,15,22,24],[23,15,23,24],[26,15,26,24],[27,15,27,24],[29,15,29,24],[28,15,28,24],[35,15,35,24],[14,1,14,4],[14,8,14,9],[17,1,17,2],[19,11,19,12],[9,5,9,6],[10,5,10,6],[32,15,32,24],[33,15,33,24],[30,15,30,24],[31,15,31,24],[15,1,15,4],[15,5,15,6],[15,8,15,9],[15,10,15,13],[15,14,15,17],[15,18,15,21],[15,22,15,24],[16,1,16,4],[16,5,16,6],[16,8,16,9],[16,10,16,13],[16,14,16,17],[16,18,16,21],[17,27,18,27],[13,18,13,21],[14,18,14,21],[8,27,8,29],[9,20,9,21],[10,23,10,26],[8,18,8,19],[8,23,8,26],[9,23,9,26],[13,25,13,26],[14,22,14,24],[15,25,15,26],[16,25,16,26],[16,22,16,24],[5,8,5,9],[6,8,6,9],[5,12,5,13],[5,10,5,11],[6,16,6,17],[10,11,10,12],[11,7,11,10],[11,11,11,14],[12,11,12,14],[10,8,10,9],[9,8,9,9],[7,12,7,14],[7,15,7,17],[9,11,9,12],[8,12,8,14],[8,10,8,11],[12,7,12,10],[8,7,8,9],[7,7,7,9],[6,2,6,7],[8,5,8,6],[12,3,12,6],[10,0,10,4],[12,0,12,2],[3,15,3,16],[24,11,24,12],[22,11,22,12],[18,11,18,12],[8,15,8,17],[10,15,10,17],[11,15,11,26],[12,15,12,26],[14,25,14,26],[7,23,7,26],[4,22,4,23],[5,23,5,26],[4,11,4,12],[13,14,13,17],[19,15,19,24],[20,15,20,24],[14,14,14,17],[7,18,7,19],[20,11,20,12],[6,12,6,13],[9,15,9,17],[6,10,6,11],[17,15,18,24],[13,22,13,24],[33,11,33,12],[29,8,29,9],[31,8,31,9],[31,11,31,12],[17,11,17,12],[20,8,20,9],[18,8,18,9],[21,11,21,12],[21,8,21,9],[28,8,28,9],[32,8,32,9],[32,11,32,12],[25,11,25,12],[30,8,30,9],[30,11,30,12],[26,11,26,12],[27,11,27,12],[25,8,25,9],[27,8,27,9],[26,8,26,9],[23,11,23,12],[24,8,24,9],[22,8,22,9],[23,8,23,9],[6,0,6,1],[7,20,7,21],[11,0,11,2],[6,23,6,26],[7,10,7,11],[17,7,17,9],[17,5,17,6],[13,8,13,9],[13,5,13,6],[14,5,14,6],[11,3,11,6],[13,1,13,4],[17,3,17,4],[9,0,9,4],[14,10,14,13],[13,10,13,13],[5,20,5,21],[5,16,5,17],[0,22,0,23],[36,8,36,9],[36,11,36,12],[36,15,36,24],[37,8,37,9],[37,11,37,12],[37,15,37,24],[1,22,1,23],[2,22,2,23],[3,22,3,23],[1,17,1,18],[0,24,1,26],[2,24,3,26],[4,24,4,26],[35,8,35,9],[35,11,35,12],[33,8,33,9],[28,11,28,12],[19,8,19,9],[34,8,34,9],[34,11,34,12],[29,11,29,12]]}
["ALS",{"$f":"AC1","v":19.023},"FHI","Fugro Geospatial",null,null,null,{"$f":"B1","v":19.023},null,"Lift Begin",null,null,null,null,"Lift End",null,null,null,null,"Flt","Flt ","Hobbs",null,null," ALS",null,null,"AO80-44-00-02",19.023,"2019-01-23","Jerry"]
[null,null,null,null,null,null,null,null,null,"Airport",null,"Chocks",null,"Hobbs","Airport","Chocks",null,"Hobbs",null,"Duration","Hrs","Hrs","   Actvity",null,null,null,null,"ISO #","Ver","Date","By"]
[null,null,null,null,null,null,null,null,1,"KMLU",null,"12:31:37",null,1449.4,"KMLU","17:46:55",null,1454.1,null,{"$f":"IF(P3=\"\",\"\",IF(P3<L3,P3+1,P3)-L3)","v":"05:15:18"},{"$f":"IF(T3=\"\",\"\",(INT(((INT(T3*1440+1/60))+7)/15)*15)/60)","v":5.25},{"$f":"IF(R3=\"\",\"\",R3-N3)","v":4.6999999999998181},"0900-Production",null,"Flight Log"]
[null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(P4=\"\",\"\",IF(P4<L4,P4+1,P4)-L4)","v":""},{"$f":"IF(T4=\"\",\"\",(INT(((INT(T4*1440+1/60))+7)/15)*15)/60)","v":""},{"$f":"IF(R4=\"\",\"\",R4-N4)","v":""}]
[null,null,null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(P5=\"\",\"\",IF(P5<L5,P5+1,P5)-L5)","v":""},{"$f":"IF(T5=\"\",\"\",(INT(((INT(T5*1440+1/60))+7)/15)*15)/60)","v":""},{"$f":"IF(R5=\"\",\"\",R5-N5)","v":""},null,null,"AO80-44-00-02"]
["FGI Job #",null,"Project Name",null,null,null,null,null,"System",null,"Unit",null,"IMU",null,"PiA","SW1","SW2-Gain",null,"Aper","AutoScan","Ground Temp°C",null,"Min Range Gate","Data Logger Drive"]
["04.33780163",null,"CPRA LADOTD",null,null,null,null,null,"ALS80",null,130,null,"uIRS",null,6,null,"",null,60,"Yes",18,29,"2657m","LG 100"]
["Flight Date",null,"GPS Day",null,"Lift",null,null,null,null,null,"Sun°",null,"Solar Times (UTC)",null,null,"Laser Power",null,null,"Pattern",null,"Flying Temp °C",null,"Max Range Gate","Download Drive"]
["2019-05-15",null,{"$f":"IF(ISBLANK(A9),\" \",CONCATENATE(TEXT(MOD(YEAR(A9),100),\"00\"),\"-\",TEXT(INT(A9)+1-DATEVALUE(CONCATENATE(\"1-Jan-\",YEAR(A9))),\"000\")))","v":"19-135"},null,8,null,null,null,null,null,"N/A",null,"N/A",null,null,1,null,null,"Triangle",null,5,5,"2931m","NS1TB-57"]
["Mission ID    (yymmdd_Sen_Job_Lift)",null,null,null,null,"Aircraft",null,"Airport ID","FMS",null,"UTC","AMT (ft)",null,"Speed","Scan Hz","Pulse Rate",null,null,"FOV","km/WPT","Altm Setting",null,null,"Shipping Track"]
["190515_130_33780163_08",null,null,null,null,"N97HC",null,"KMLU","CCNS 4",null,"",9101,null,150,53,610000,null,null,29,1.6679999999999999,30.02,30.04,null,"7752 2787 4882"]
["Pilot #1",null,null,"Pilot #2",null,null,null,"Operator #1",null,null,null,"Operator #2"]
["George Jordan",null,null,"",null,null,null,"Dave Verhey",null,null,null,""]
["Base 1 ID","Location",null,null,null,"Rec ID",null,"Ant ID","ARP (m)",null,"Start Time (UTC)",null,null,null,"Stop Time (UTC)",null,null,null,"GPS Filename",null,null,null,"Operator",null,null,"Data"]
["FUG-KMLU","KMLU",null,null,null,"GR3 U1",null,"U1",1.8,null,"2019-05-15T12:19:00",null,null,null,"2019-05-15T18:08:00",null,null,null,"unit10515m",null,null,null,"Dave Verhey",null,null,"FTP"]
["Base 2 ID","Location",null,null,null,"Rec ID",null,"Ant ID","ARP (m)",null,"Start Time (UTC)",null,null,null,"Stop Time (UTC)",null,null,null,"GPS Filename",null,null,null,"Operator",null,null,"Data"]
["LARU","LARU",null,null,null,"",null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,"CORS",null,null,""]
["   ","Flight #",null,"Wpt",null,"Distance",null,"UTC",null,null,"Flt","Altitude",null,"Speed","Scan","Comments and Conditions",null,null,null,null,null,null,null,null,null,"   ",null,"OnLine Time"]
["Area","FGI","Client's","From","To","Begin","End","Start","End",null,"Dir","(GPS)",null,"(knots)","Rate",null,null,null,null,null,null,null,null,null,null,"SVs","PDOP"]
[null,null,null,null,null,null,null,"12:35:19","12:40:19",null,null,null,null,null,null,"Ground Static at KMLU",null,null,null,null,null,null,null,null,null,19,1.5,{"$f":"IF(H20=\"\",0,IF(I20=\"\",0,I20-H20))","v":"00:05:00"}]
[null,null,null,null,null,null,null,"13:09:11","13:11:19",null,null,null,null,null,null,"S-Turn",null,null,null,null,null,null,null,null,null,23,1.1000000000000001,{"$f":"IF(H21=\"\",0,IF(I21=\"\",0,I21-H21))","v":"00:02:08"}]
["LA_1X",9,null,41,31,66.400000000000006,50,"13:13:24","13:14:39",null,"269.6",9156,null,146,null,"Tie line; track edge exceeded while observing traffic. Restart line",null,null,null,null,null,null,null,null,null,23,1.1000000000000001,"00:01:15"]
["LA_1X",9,null,41,31,66.400000000000006,50,"13:19:30","13:23:09",null,"269.6",9156,null,145,null,"Tie line; IP missed-- laser manually fired within wp 38 instead.",null,null,null,null,null,null,null,null,null,23,1.2,"00:03:39"]
["LA_1B",11,null,54,1,88.4,0,"13:28:31","13:49:42",null,"179.2",9204,null,136,null,"Water 63-59 km",null,null,null,null,null,null,null,null,null,22,1.2,"00:21:11"]
[null,12,null,1,54,0,88.4,"13:52:44","14:12:49",null,"359.2",9210,null,145,null,"Water 59-63.5 km",null,null,null,null,null,null,null,null,null,21,1.1000000000000001,"00:20:05"]
[null,13,null,54,1,88.4,0,"14:15:58","14:35:52",null,"179.3",9170,null,147,null,"Water 63.5-57.5 km",null,null,null,null,null,null,null,null,null,21,1.2,"00:19:54"]
[null,13,null,1,10,0,15,"14:39:14","14:42:50",null,"359.2",9190,null,144,null,"Calibration line",null,null,null,null,null,null,null,null,null,22,1.1000000000000001,"00:03:36"]
[null,14,null,1,54,0,88.4,"14:50:09","15:10:03",null,"359.2",9182,null,140,null,"Water 51, 57.5-64 km",null,null,null,null,null,null,null,null,null,19,1.2,"00:19:54"]
[null,15,null,54,1,88.4,0,"15:13:35","15:33:31",null,"179.3",9191,null,148,null,"Course correction 7 km; Water 66.5, 62.5-57.5 km",null,null,null,null,null,null,null,null,null,22,1.2,"00:19:56"]
[null,16,null,1,54,0,88.4,"15:36:52","15:56:30",null,"359.2",9241,null,144,null,"Water 13.5, 57-63, 67, 82 km",null,null,null,null,null,null,null,null,null,21,1.2,"00:19:38"]
[null,17,null,54,1,88.4,0,"15:59:37","16:19:42",null,"179.3",9143,null,144,null,"Water 62-56, 46.5, 29.5 km",null,null,null,null,null,null,null,null,null,23,1.1000000000000001,"00:20:05"]
[null,18,null,1,54,0,88.4,"16:23:26","16:43:04",null,"359.2",9193,null,140,null,"Water 56.5,59-62.5 km",null,null,null,null,null,null,null,null,null,23,1.2,"00:19:38"]
[null,19,null,54,1,88.4,0,"16:45:43","17:05:24",null,"179.3",9172,null,144,null,"Course correction 77 km; Cloud 65.5 km; water 60.5-54 km; possible flooding 12 km; course correction 6 km",null,null,null,null,null,null,null,null,null,22,1.2,"00:19:41"]
[null,null,null,null,null,null,null,"17:05:32","17:07:13",null,null,null,null,null,null,"S-Turn",null,null,null,null,null,null,null,null,null,21,1.1000000000000001,"00:01:41"]
[null,null,null,null,null,null,null,"17:15:09","17:20:09",null,null,null,null,null,null,"Overflight of CORS at LARU (learned site was not usable post-flight)",null,null,null,null,null,null,null,null,null,20,1.3,"00:05:00"]
[null,null,null,null,null,null,null,"17:39:00","17:44:00",null,null,null,null,null,null,"Ground Static at KMLU",null,null,null,null,null,null,null,null,null,20,1.2,"00:05:00"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H37=\"\",0,IF(I37=\"\",0,I37-H37))","v":"00:00:00"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H38=\"\",0,IF(I38=\"\",0,I38-H38))","v":"00:00:00"}]