

**Michigan LiDAR 2016 – Roscommon**

**LiDAR Correction Response**

May 11, 2017

**Summary**

This document gives an overview of the corrections made to the Roscommon products.

**Metadata**

-Metadata and accuracy report included.

**Raw Swath LAS**

-All header information is fixed. Intensity values are scaled correctly.

**Classified LAS**

-All header information is fixed. Intensity values are scaled correctly. 3 files are missing due to empty tiles over water.

**Breaklines**

-Breaklines included.

**DEM**

-1 valid correction was addressed and fixed. Shapefile included.