

**Michigan LiDAR 2015 – St. Joseph**

**LiDAR Correction Response**

 August 1, 2017

**Summary**

This document gives an overview of the corrections made to the St. Joseph LiDAR products.

**Raw LAS**

-Scan direction bit data is unrecoverable due to a software version problem.

**DEM**

-All remaining islands are under 1 acre per spec. No corrections needed.