Please note that this project has some significant divergences from the task order in terms of tile layout and spatial reference for the two AOI's in the task order.  It was determined that we wouldn't do a modification to the task order for this however.  So please see the notes below on the pertinent differences.  I have also attached a draft non-official modification that may be better to use than the original awarded task order for the QA of this project (differences are noted in Red Text). Iv'e also noted this information in the attached QA report as well in the Geographic Information section.  Pleased feel free to contact me if you have any questions relating to all this.

Northern AOI

         NAD83(2011) UTM Zone 16, Meters

         NAVD88 Geoid 12b, Meters

         1500m x 1500m Tiles

         Tiles to be named following the US National Grid

1 Meter DEM cells

Southern AOI

         NAD83(2011) State Plane Coordinate System Mississippi East, US Survey Feet

         NAVD88 Geoid 12b, US Survey Feet

         5000ft x 5000ft Tiles

         Tiles to be named using the xy coordinates of the lower left corner

2.5 Ft. DEM cells

thank you,

Jayna