**Explanation of Edit Calls**

All edit calls were addressed and noted with the appropriate action taken in the shapefile.

**Explanation of Data Void**

The original tile layout supplied by the state of North Carolina did not contain these tiles due to them being 100% in water. PSI has gone ahead and created these 2 tiles in order to fill the data void. LAS Files, DEMs, and Intensity Images were all created due to this.

**Raw Swath Data Not Accepted**

These files were not accepted due to the swath being greater than 2 GB in size. PSI received a waiver on this.

**Min Scan Angle exceeds -37.5**

The minimum scan angle on 3 tiles exceeds -37.5. Upon further review, it was determined that the affected points did not affect the data adversely and so no corrective action was taken. 2 of the 3 tiles (LA\_37\_20467102 and LA\_37\_20467104) only had a total of 4 points that fell within this range.